PRISM_DATASET_FILENAME: prism_solslope_us_25m_1921.tif
PRISM_DATASET_CREATE_DATE: 20260213-1225
PRISM_SOURCE_FILENAME: topo_gsolar_slope_us_us_30s_192101.bil, topo_gsolar_slope_us_us_30s_192102.bil, topo_gsolar_slope_us_us_30s_192103.bil, topo_gsolar_slope_us_us_30s_192104.bil, topo_gsolar_slope_us_us_30s_192105.bil, topo_gsolar_slope_us_us_30s_192106.bil, topo_gsolar_slope_us_us_30s_192107.bil, topo_gsolar_slope_us_us_30s_192108.bil, topo_gsolar_slope_us_us_30s_192109.bil, topo_gsolar_slope_us_us_30s_192110.bil, topo_gsolar_slope_us_us_30s_192111.bil, topo_gsolar_slope_us_us_30s_192112.bil
PRISM_SOURCE_CREATE_DATE: 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406, 20251120-1406
PRISM_DATASET_TYPE: an91/r2112
PRISM_DATASET_VERSION: M3
PRISM_CODE_VERSION: 16.2-20250715-1813
PRISM_DATASET_RELEASE_NUMBER: 2
PRISM_DATASET_REMARKS: This grid was developed in three steps: (1) solar data were modeled with PRISM at 30-arc-second (~800m) resolution to produce the source grid(s) listed under PRISM_SOURCE_FILENAME, on the date(s) listed under PRISM_SOURCE_CREATE_DATE; (2) These twelve monthly 800m grids were then upscaled to 2.5-arc-minute(~ 4km) resolution with a Gaussian filter; and (3) The resulting twelve monthly 4km grids were averaged to obtain a 4km mean annual solar grid.
